# OGGETTO: FORNITURA DI UN SISTEMA STORAGE NETAPP METROCLUSTER

# Codice appalto: 29468

# CIG n. 7768144B36

Il sottoscritto Concorrente \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ con sede legale in \_\_\_\_\_\_\_\_\_\_\_\_\_\_, Via/Piazza \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ n. \_\_\_\_ - cap. \_\_\_\_\_\_\_\_\_ città \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ provincia di \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, C.F. n. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ partita I.V.A. n. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ed inscritta alla C.C.I.A.A. di \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ con il n. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ [*N.B.: in caso di raggruppamenti/aggregazioni di imprese indicare i riferimenti della mandataria e delle mandanti*]

**OFFRE**

sotto la sua responsabilità civile e penale ai sensi del D.P.R. n. 445/2000 e s.m.i., i seguenti importi unitari e complessivi:

| **n.** | **Codice** | **Descrizione beni** | **Q.ta** | **Prezzo unitario** | **Importo** |
| --- | --- | --- | --- | --- | --- |
| 1 | AFF-A300A-001 | AFF A300 HA System,FlashBundle Includes All Protocols, SnapRestore, SnapMirror, SnapVault, FlexClone, SnapManager Suite, Single Mailbox Recovery (SMBR), SnapCenter Foundation. | 2 |  |  |
| 2 | X1144A-C | NIC 2-Port Bare Cage 40GbE QSFP+ PCIe,-C | 2 |  |  |
| 3 | X1133A-R6-C | HBA,4-Port FCP Trgt/Init 16Gb PCIe w/SFP+,-C | 2 |  |  |
| 4 | X66250-5-C | Cable,LC-LC,OM4,5m,-C | 24 |  |  |
| 5 | X66032A-C | Cable,12Gb,Mini SAS HD,2m,-C | 4 |  |  |
| 6 | X66200-5-C | Cable,Cntlr-Switch OM4,MPO/MPO,5m,-C | 4 |  |  |
| 7 | X6235-C | Chassis,FAS8200,AFF-A300,AC PS,-C | 2 |  |  |
| 8 | DOC-AFF-A300-C | Documents,AFF-A300,-C | 2 |  |  |
| 9 | X1985-R6-C | 12-Node Cluster Cable Label Kit,-C | 2 |  |  |
| 10 | X870F-C | Cabinet,1280mm,Empty,No PDU,No Rails,-C | 2 |  |  |
| 11 | X6596-R6-C | SFP+ FC Optical 16Gb,-C | 8 |  |  |
| 12 | X65402-C | QSFP,Opt,40Gb,Shortwave,-C | 4 |  |  |
| 13 | X1613A-MC-C | Bridge,ATTO 7500N FC-SAS,-C | 4 |  |  |
| 14 | X87880A-C | Rail Kit 4,Cabinet,-C | 8 |  |  |
| 15 | X800-42U-R6-C | Power Cable,In-Cabinet,C13-C14,-C | 4 |  |  |
| 16 | X1558A-R6-C | Power Cable,In-Cabinet,48-IN,C13-C14,-C | 12 |  |  |
| 17 | X800-42U-43-C | Power Cable,In-Cabinet,C13-C14,43-inch,-C | 4 |  |  |
| 18 | X8713C-EN-R6-C | PDU,1-Phase,12 Outlet,30A,IEC,EN,-C,R6 | 8 |  |  |
| 19 | X87007A-C | Rear Tie Down Bracket,Short Chassis,Cab,-C | 2 |  |  |
| 20 | ALL-FLASH-OPTIMIZED | Optimized SSD Personality | 1 |  |  |
| 21 | X-000072-R6-C | Kit,Brocade 300/6510/67XX Rackmount Rail,-C | 4 |  |  |
| 22 | X-G610-24-16G-1-MC-C | Switch,Brocade G610 24-Pt w/16Gb SWL SFP+Ent ( Includes 24 16G SWL SFPs and Enterprise SW ) | 4 |  |  |
| 24 | DS224C-SL-3.8-24S-2P-C | SSD Shelf,12G,24x3.8TB,2P,-C | 2 |  |  |
| 25 | SW-2-A300A-NVE-C | SW,Data at Rest Encryption Enabled,A300A,-C | 2 |  |  |
| 26 | SW-2-A300A-TPM-C | SW,Trusted Platform Module Enabled,A300A,-C | 2 |  |  |
| 27 | SW-2-CL-BASE | SW-2,Base,CL,Node | 2 |  |  |
| 28 | DATA-AT-REST-ENCRYPTION | Data at Rest Encryption Capable Operating Sys | 2 |  |  |
| 29 | SW-FLASH-BUNDLE-2P-C | ONTAP,Per-0.1TB,FlashBundle,Ult-Perf,2P,-C | 1824 |  |  |
| 30 | SW-BSW-NTWADV-SANPLU-MC-C | SW,Brocade Pro Plus Lic for MC,-C | 1 |  |  |
| 31 | CS-O2-NOINSTALL-4HR | SupportEdge Premium 4hr Onsite, w/o Install | 1 |  |  |
| 32 | X8781-R6 | Hardware Kit,Add-On Peripheral,Cabinet,R6 | 1 |  |  |
| 33 | X8781-R6 | Hardware Kit,Add-On Peripheral,Cabinet,R6 | 1 |  |  |
| 34 | X66032A | Cable,12Gb,Mini SAS HD,2m | 4 |  |  |
| 35 | X66032A | Cable,12Gb,Mini SAS HD,2m | 4 |  |  |
| 36 | X800-42U-35 | Power Cable,In-Cabinet,C13-C14,35-inch | 2 |  |  |
| 37 | X800-42U-35 | Power Cable,In-Cabinet,C13-C14,35-inch | 2 |  |  |
| 38 | DS224C-SL-3.8-12S-QS | SSD Shelf,12G,12x3.8TB,-QS OS Ultra-Performance (TB): 45.6 | 1 |  |  |
| 39 | DS224C-S-.96-12S-QS | SSD Shelf,12G,12x960GB,-QS OS Ultra-Performance (TB): 11.5 | 1 |  |  |
| 40 | SW-FLASHBNDL-ADD-2P-QS | ONTAP,Per-0.1TB,FlashBundle,Add-On,2P,QS | 456 |  |  |
| 41 | SW-FLASHBNDL-ADD-2P-QS | ONTAP,Per-0.1TB,FlashBundle,Add-On,2P,QS | 115 |  |  |
| 42 | CS-INSTALL | Base Installation Service Period Duration: 1 Month Service Address: Via Giovanni Bovio 23 Calenzano 50041 | 1 |  |  |
| 43 | CS-INSTALL | Base Installation Service Period Duration: 1 Month Service Address: Via Giovanni Bovio 23 Calenzano 50041 | 1 |  |  |
| 44 | CS-O2-4HR | SupportEdge Premium 4hr Onsite Service Period Duration:36 Month Service Address: Via Giovanni Bovio 23 Calenzano 50041 | 1 |  |  |
| 45 | CS-O2-4HR | SupportEdge Premium 4hr Onsite Service Period Duration:36 Month Service Address: Via Giovanni Bovio 23 Calenzano 50041 | 1 |  |  |
| 46 | X1558A-R6 | Power Cable,In-Cabinet,48-IN,C13-C14 | 8 |  |  |
| 47 | X6599A-R6 | SFP+ Optical 10Gb Shortwave | 4 |  |  |
| 48 | X66205-5 | Cable,Cntlr-Switch OM4,MPO/4x10G LC,5m | 2 |  |  |
| 49 | X357A | SSD,3.8TB,12G,DS224C,W/MSW | 6 |  |  |
| **Importo complessivo offerto (A)** | | | | **\_\_\_\_\_\_\_\_\_ €** | |
| **Pari ad un ribasso sulla base d’asta di (B):** | | | | **\_\_\_\_\_\_\_\_\_ %** | |

Tutti gli importi sono al netto di Iva e/o di altre imposte e contributi di legge, nonché degli oneri per la sicurezza dovuti a rischi da interferenze.

***Documento informatico firmato digitalmente ai sensi del D.Lgs 82/2005 s.m.i. e norme collegate, il quale sostituisce il documento cartaceo e la firma autografa.***